(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "Device:Q_NPN_BEC" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Q" (id 0) (at 5.08 1.27 0))
      (property "Value" "Q_NPN_BEC" (id 1) (at 5.08 -1.27 0))
      (property "Footprint" "" (id 2) (at 5.08 2.54 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "transistor NPN" (id 4) (at 0 0 0))
      (property "ki_description" "NPN transistor, base/emitter/collector" (id 5) (at 0 0 0))
      (symbol "Q_NPN_BEC_0_1"
        (polyline
          (pts
            (xy 0.635 0.635)
            (xy 2.54 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 -0.635)
            (xy 2.54 -2.54)
            (xy 2.54 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 1.905)
            (xy 0.635 -1.905)
            (xy 0.635 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.778)
            (xy 1.778 -1.27)
            (xy 2.286 -2.286)
            (xy 1.27 -1.778)
            (xy 1.27 -1.778)
          )
          (fill (type outline))
        )
        (circle (center 1.27 0) (radius 2.8194)
          (fill (type none))
        )
      )
      (symbol "Q_NPN_BEC_1_1"
        (pin input line (at -5.08 0 0) (length 5.715)
          (name "B")
          (number "1")
        )
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "E")
          (number "2")
        )
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "C")
          (number "3")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
    (symbol "pyopus:OUTPUT_FILE" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "A" (id 0) (at -10.16 1.27 0))
      (property "Value" "OUTPUT_FILE" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "Name" "<file name>" (id 4) (at -10.16 -6.35 0))
      (property "ki_description" "Define subcircuit" (id 5) (at 0 0 0))
      (symbol "OUTPUT_FILE_0_1"
        (rectangle (start -10.16 0) (end 10.16 -5.08)
          (fill (type none))
        )
      )
    )
    (symbol "pyopus:VSRC" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "V" (id 0) (at -3.81 0 90))
      (property "Value" "VSRC" (id 1) (at -6.35 0 90))
      (property "Footprint" "" (id 2) (at -6.858 -19.05 90))
      (property "Datasheet" "" (id 3) (at -5.08 -19.05 90))
      (property "Specification" "dc=0" (id 4) (at 3.81 0 90))
      (property "ki_description" "Built-in independent voltage source" (id 5) (at 0 0 0))
      (symbol "VSRC_0_0"
        (circle (center 0 0) (radius 1.905)
          (fill (type none))
        )
        (text "+" (at 0 1.27 0))
        (text "-" (at 0 -1.27 0))
      )
      (symbol "VSRC_1_1"
        (pin passive line (at 0 3.81 270) (length 1.905)
          (name "P")
          (number "1")
        )
        (pin power_out line (at 0 -3.81 90) (length 1.905)
          (name "N")
          (number "2")
        )
      )
    )
  )
  (junction (at 104.14 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 119.38 81.28) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 104.14 86.36) (xy 111.76 86.36)))
  (wire (pts (xy 119.38 78.74) (xy 119.38 81.28)))
  (wire (pts (xy 104.14 83.82) (xy 104.14 86.36)))
  (wire (pts (xy 119.38 81.28) (xy 140.97 81.28)))
  (global_label "c4" (shape input) (at 119.38 78.74 90) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 0 0 0))
  )
  (global_label "b4" (shape input) (at 104.14 83.82 90) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 0 0 0))
  )
  (symbol (lib_id "pyopus:OUTPUT_FILE") (at 110.49 62.23 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "A1" (id 0) (at 100.33 60.96 0))
    (property "Value" "" (id 1) (at 110.49 64.77 0))
    (property "Footprint" "" (id 2) (at 110.49 62.23 0))
    (property "Datasheet" "" (id 3) (at 110.49 62.23 0))
    (property "Name" "netlister.cir" (id 4) (at 100.33 68.58 0))
  )
  (symbol (lib_id "pyopus:VSRC") (at 104.14 90.17 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Vbe4" (id 0) (at 100.33 90.17 90))
    (property "Value" "" (id 1) (at 97.79 90.17 90))
    (property "Footprint" "" (id 2) (at 97.282 109.22 90))
    (property "Datasheet" "" (id 3) (at 99.06 109.22 90))
    (property "Specification" "dc=0" (id 4) (at 107.95 90.17 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pyopus:VSRC") (at 140.97 85.09 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Vce4" (id 0) (at 137.16 85.09 90))
    (property "Value" "" (id 1) (at 134.62 85.09 90))
    (property "Footprint" "" (id 2) (at 134.112 104.14 90))
    (property "Datasheet" "" (id 3) (at 135.89 104.14 90))
    (property "Specification" "dc=0" (id 4) (at 144.78 85.09 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 104.14 93.98 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0101" (id 0) (at 104.14 100.33 0))
    (property "Value" "" (id 1) (at 104.14 97.79 0))
    (property "Footprint" "" (id 2) (at 104.14 93.98 0))
    (property "Datasheet" "" (id 3) (at 104.14 93.98 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 140.97 88.9 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0102" (id 0) (at 140.97 95.25 0))
    (property "Value" "" (id 1) (at 140.97 92.71 0))
    (property "Footprint" "" (id 2) (at 140.97 88.9 0))
    (property "Datasheet" "" (id 3) (at 140.97 88.9 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 119.38 91.44 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0103" (id 0) (at 119.38 97.79 0))
    (property "Value" "" (id 1) (at 119.38 95.25 0))
    (property "Footprint" "" (id 2) (at 119.38 91.44 0))
    (property "Datasheet" "" (id 3) (at 119.38 91.44 0))
    (pin "1")
  )
  (symbol (lib_id "Device:Q_NPN_BEC") (at 116.84 86.36 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Q1" (id 0) (at 121.92 85.09 0))
    (property "Value" "" (id 1) (at 121.92 87.63 0))
    (property "Footprint" "" (id 2) (at 121.92 83.82 0))
    (property "Datasheet" "~" (id 3) (at 116.84 86.36 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "#PWR0101") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0102") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0103") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "A1") (unit 1) (value "OUTPUT_FILE") (footprint "")
    )
    (path
      (reference "Q1") (unit 1) (value "Q_NPN_BEC") (footprint "")
    )
    (path
      (reference "Vbe4") (unit 1) (value "VSRC") (footprint "")
    )
    (path
      (reference "Vce4") (unit 1) (value "VSRC") (footprint "")
    )
  )
)
