(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "pyopus:CAP" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at -3.81 0 90))
      (property "Value" "CAP" (id 1) (at -6.35 0 90))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 90))
      (property "Datasheet" "" (id 3) (at -3.81 0 90))
      (property "c" "<capacitance>" (id 4) (at 3.81 0 90))
      (property "ki_description" "Built-in capacitor" (id 5) (at 0 0 0))
      (symbol "CAP_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "CAP_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "pyopus:INCLUDE" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "A" (id 0) (at -10.16 1.27 0))
      (property "Value" "INCLUDE" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "Filename" "<file name>" (id 4) (at -10.16 -6.35 0))
      (property "Position" "top" (id 5) (at 10.16 1.27 0))
      (property "ki_description" "Include file" (id 6) (at 0 0 0))
      (symbol "INCLUDE_0_1"
        (rectangle (start -10.16 0) (end 10.16 -5.08)
          (fill (type none))
        )
      )
    )
    (symbol "pyopus:ISRC" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "I" (id 0) (at -3.81 0 90))
      (property "Value" "ISRC" (id 1) (at -6.35 0 90))
      (property "Footprint" "" (id 2) (at -6.858 -19.05 90))
      (property "Datasheet" "" (id 3) (at -5.08 -19.05 90))
      (property "Specification" "dc=0" (id 4) (at 3.81 0 90))
      (property "ki_description" "Built-in independent current source" (id 5) (at 0 0 0))
      (symbol "ISRC_0_0"
        (polyline
          (pts
            (xy 0 1.143)
            (xy 0 -1.143)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -1.143)
            (xy -0.254 -0.381)
            (xy 0.254 -0.381)
            (xy 0 -1.143)
          )
          (fill (type none))
        )
        (circle (center 0 0) (radius 1.905)
          (fill (type none))
        )
      )
      (symbol "ISRC_1_1"
        (pin passive line (at 0 3.81 270) (length 1.905)
          (name "P")
          (number "1")
        )
        (pin power_out line (at 0 -3.81 90) (length 1.905)
          (name "N")
          (number "2")
        )
      )
    )
    (symbol "pyopus:NMOS" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "M" (id 0) (at 5.08 5.08 0))
      (property "Value" "NMOS" (id 1) (at 5.08 7.62 0))
      (property "Footprint" "" (id 2) (at 5.08 7.62 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "Model" "<model name>" (id 4) (at 5.08 2.54 0))
      (property "w" "<w>" (id 5) (at -1.27 5.08 0))
      (property "l" "<l>" (id 6) (at -1.27 2.54 0))
      (property "m" "<m>" (id 7) (at -1.27 -3.81 0))
      (property "ki_description" "Built-in NMOS transistor" (id 8) (at 0 0 0))
      (symbol "NMOS_0_1"
        (polyline
          (pts
            (xy 0.762 -1.778)
            (xy 2.54 -1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 -1.27)
            (xy 0.762 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 0)
            (xy 2.54 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 0.508)
            (xy 0.762 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 1.778)
            (xy 2.54 1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 2.286)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -1.778)
            (xy 2.54 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 2.54)
            (xy 2.54 1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.254 1.905)
            (xy 0.254 -1.905)
            (xy 0.254 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 0)
            (xy 2.032 0.381)
            (xy 2.032 -0.381)
            (xy 1.016 0)
          )
          (fill (type outline))
        )
        (circle (center 2.54 -1.778) (radius 0.2794)
          (fill (type outline))
        )
        (circle (center 2.54 1.778) (radius 0.2794)
          (fill (type outline))
        )
      )
      (symbol "NMOS_1_1"
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "D")
          (number "1")
        )
        (pin input line (at -5.08 0 0) (length 5.334)
          (name "G")
          (number "2")
        )
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "S")
          (number "3")
        )
        (pin input line (at 6.35 0 180) (length 5.08)
          (name "B")
          (number "4")
        )
      )
    )
    (symbol "pyopus:OUTPUT_FILE" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "A" (id 0) (at -10.16 1.27 0))
      (property "Value" "OUTPUT_FILE" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "Name" "<file name>" (id 4) (at -10.16 -6.35 0))
      (property "ki_description" "Define subcircuit" (id 5) (at 0 0 0))
      (symbol "OUTPUT_FILE_0_1"
        (rectangle (start -10.16 0) (end 10.16 -5.08)
          (fill (type none))
        )
      )
    )
    (symbol "pyopus:PMOS" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "M" (id 0) (at 5.08 5.08 0))
      (property "Value" "PMOS" (id 1) (at 5.08 7.62 0))
      (property "Footprint" "" (id 2) (at 5.08 6.35 0))
      (property "Datasheet" "" (id 3) (at 5.08 5.08 0))
      (property "Model" "<model name>" (id 4) (at 5.08 2.54 0))
      (property "w" "<w>" (id 5) (at -1.27 5.08 0))
      (property "l" "<l>" (id 6) (at -1.27 2.54 0))
      (property "m" "<m>" (id 7) (at -1.27 -3.81 0))
      (property "ki_description" "Built-in PMOS transistor" (id 8) (at 0 0 0))
      (symbol "PMOS_0_1"
        (polyline
          (pts
            (xy 0.762 -1.778)
            (xy 2.54 -1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 -1.27)
            (xy 0.762 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 0)
            (xy 2.54 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 0.508)
            (xy 0.762 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 1.778)
            (xy 2.54 1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 2.286)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -1.778)
            (xy 2.54 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 2.54)
            (xy 2.54 1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.254 1.905)
            (xy 0.254 -1.905)
            (xy 0.254 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.286 0)
            (xy 1.27 -0.381)
            (xy 1.27 0.381)
            (xy 2.286 0)
          )
          (fill (type outline))
        )
        (circle (center 2.54 -1.778) (radius 0.2794)
          (fill (type outline))
        )
        (circle (center 2.54 1.778) (radius 0.2794)
          (fill (type outline))
        )
      )
      (symbol "PMOS_1_1"
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "D")
          (number "1")
        )
        (pin input line (at -5.08 0 0) (length 5.334)
          (name "G")
          (number "2")
        )
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "S")
          (number "3")
        )
        (pin input line (at 6.35 0 180) (length 5.08)
          (name "B")
          (number "4")
        )
      )
    )
    (symbol "pyopus:RES" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at -2.54 0 90))
      (property "Value" "RES" (id 1) (at -5.08 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "" (id 3) (at 2.032 0 90))
      (property "r" "<resistance>" (id 4) (at 2.54 0 90))
      (property "ki_keywords" "r res resistor" (id 5) (at 0 0 0))
      (property "ki_description" "Built-in resistor" (id 6) (at 0 0 0))
      (symbol "RES_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "RES_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "pyopus:SUBCKT" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "A" (id 0) (at -10.16 1.27 0))
      (property "Value" "SUBCKT" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "Name" "<name>" (id 4) (at -10.16 -6.35 0))
      (property "Pins" "<pin names>" (id 5) (at -10.16 -8.89 0))
      (property "ki_description" "Define subcircuit" (id 6) (at 0 0 0))
      (symbol "SUBCKT_0_1"
        (rectangle (start -10.16 0) (end 10.16 -5.08)
          (fill (type none))
        )
      )
    )
  )
  (junction (at 151.13 74.93) (diameter 0) (color 0 0 0 0))
  (junction (at 64.77 125.73) (diameter 0) (color 0 0 0 0))
  (junction (at 110.49 142.24) (diameter 0) (color 0 0 0 0))
  (junction (at 88.9 125.73) (diameter 0) (color 0 0 0 0))
  (junction (at 64.77 142.24) (diameter 0) (color 0 0 0 0))
  (junction (at 116.84 74.93) (diameter 0) (color 0 0 0 0))
  (junction (at 110.49 111.76) (diameter 0) (color 0 0 0 0))
  (junction (at 106.68 142.24) (diameter 0) (color 0 0 0 0))
  (junction (at 151.13 99.06) (diameter 0) (color 0 0 0 0))
  (junction (at 151.13 142.24) (diameter 0) (color 0 0 0 0))
  (junction (at 102.87 120.65) (diameter 0) (color 0 0 0 0))
  (junction (at 130.81 99.06) (diameter 0) (color 0 0 0 0))
  (junction (at 80.01 125.73) (diameter 0) (color 0 0 0 0))
  (junction (at 116.84 99.06) (diameter 0) (color 0 0 0 0))
  (junction (at 85.09 74.93) (diameter 0) (color 0 0 0 0))
  (junction (at 64.77 74.93) (diameter 0) (color 0 0 0 0))
  (junction (at 88.9 74.93) (diameter 0) (color 0 0 0 0))
  (junction (at 120.65 74.93) (diameter 0) (color 0 0 0 0))
  (junction (at 102.87 83.82) (diameter 0) (color 0 0 0 0))
  (junction (at 88.9 93.98) (diameter 0) (color 0 0 0 0))
  (junction (at 60.96 142.24) (diameter 0) (color 0 0 0 0))
  (junction (at 102.87 142.24) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 120.65 74.93) (xy 151.13 74.93)))
  (wire (pts (xy 151.13 99.06) (xy 151.13 128.27)))
  (wire (pts (xy 88.9 133.35) (xy 95.25 133.35)))
  (wire (pts (xy 154.94 74.93) (xy 154.94 83.82)))
  (wire (pts (xy 102.87 83.82) (xy 102.87 93.98)))
  (wire (pts (xy 88.9 116.84) (xy 88.9 120.65)))
  (wire (pts (xy 102.87 93.98) (xy 88.9 93.98)))
  (wire (pts (xy 151.13 78.74) (xy 151.13 74.93)))
  (wire (pts (xy 124.46 111.76) (xy 127 111.76)))
  (wire (pts (xy 110.49 142.24) (xy 151.13 142.24)))
  (wire (pts (xy 102.87 142.24) (xy 102.87 138.43)))
  (wire (pts (xy 85.09 74.93) (xy 88.9 74.93)))
  (wire (pts (xy 80.01 125.73) (xy 88.9 125.73)))
  (wire (pts (xy 88.9 125.73) (xy 139.7 125.73)))
  (wire (pts (xy 64.77 142.24) (xy 64.77 138.43)))
  (wire (pts (xy 130.81 83.82) (xy 143.51 83.82)))
  (wire (pts (xy 110.49 111.76) (xy 113.03 111.76)))
  (wire (pts (xy 64.77 104.14) (xy 64.77 125.73)))
  (wire (pts (xy 64.77 125.73) (xy 64.77 128.27)))
  (wire (pts (xy 92.71 111.76) (xy 110.49 111.76)))
  (wire (pts (xy 88.9 120.65) (xy 102.87 120.65)))
  (wire (pts (xy 102.87 142.24) (xy 106.68 142.24)))
  (wire (pts (xy 64.77 96.52) (xy 64.77 74.93)))
  (wire (pts (xy 88.9 78.74) (xy 88.9 74.93)))
  (wire (pts (xy 85.09 83.82) (xy 85.09 74.93)))
  (wire (pts (xy 151.13 74.93) (xy 154.94 74.93)))
  (wire (pts (xy 102.87 83.82) (xy 109.22 83.82)))
  (wire (pts (xy 64.77 125.73) (xy 80.01 125.73)))
  (wire (pts (xy 130.81 99.06) (xy 132.08 99.06)))
  (wire (pts (xy 149.86 99.06) (xy 151.13 99.06)))
  (wire (pts (xy 154.94 142.24) (xy 154.94 133.35)))
  (wire (pts (xy 96.52 83.82) (xy 102.87 83.82)))
  (wire (pts (xy 116.84 88.9) (xy 116.84 99.06)))
  (wire (pts (xy 60.96 142.24) (xy 64.77 142.24)))
  (wire (pts (xy 78.74 111.76) (xy 81.28 111.76)))
  (wire (pts (xy 116.84 99.06) (xy 130.81 99.06)))
  (wire (pts (xy 60.96 133.35) (xy 60.96 142.24)))
  (wire (pts (xy 116.84 78.74) (xy 116.84 74.93)))
  (wire (pts (xy 64.77 74.93) (xy 85.09 74.93)))
  (wire (pts (xy 54.61 142.24) (xy 60.96 142.24)))
  (wire (pts (xy 80.01 133.35) (xy 80.01 125.73)))
  (wire (pts (xy 151.13 142.24) (xy 154.94 142.24)))
  (wire (pts (xy 54.61 74.93) (xy 64.77 74.93)))
  (wire (pts (xy 88.9 93.98) (xy 88.9 106.68)))
  (wire (pts (xy 139.7 133.35) (xy 143.51 133.35)))
  (wire (pts (xy 120.65 83.82) (xy 120.65 74.93)))
  (wire (pts (xy 88.9 88.9) (xy 88.9 93.98)))
  (wire (pts (xy 130.81 99.06) (xy 130.81 83.82)))
  (wire (pts (xy 116.84 99.06) (xy 116.84 106.68)))
  (wire (pts (xy 64.77 142.24) (xy 102.87 142.24)))
  (wire (pts (xy 72.39 133.35) (xy 80.01 133.35)))
  (wire (pts (xy 139.7 125.73) (xy 139.7 133.35)))
  (wire (pts (xy 102.87 120.65) (xy 116.84 120.65)))
  (wire (pts (xy 110.49 111.76) (xy 110.49 142.24)))
  (wire (pts (xy 151.13 99.06) (xy 153.67 99.06)))
  (wire (pts (xy 116.84 74.93) (xy 120.65 74.93)))
  (wire (pts (xy 151.13 142.24) (xy 151.13 138.43)))
  (wire (pts (xy 88.9 125.73) (xy 88.9 133.35)))
  (wire (pts (xy 139.7 99.06) (xy 142.24 99.06)))
  (wire (pts (xy 106.68 142.24) (xy 110.49 142.24)))
  (wire (pts (xy 106.68 142.24) (xy 106.68 133.35)))
  (wire (pts (xy 88.9 74.93) (xy 116.84 74.93)))
  (wire (pts (xy 116.84 120.65) (xy 116.84 116.84)))
  (wire (pts (xy 102.87 128.27) (xy 102.87 120.65)))
  (wire (pts (xy 151.13 88.9) (xy 151.13 99.06)))
  (global_label "vdd" (shape input) (at 54.61 74.93 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 0 0 0))
  )
  (global_label "out" (shape input) (at 153.67 99.06 0) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 0 0 0))
  )
  (global_label "vss" (shape input) (at 54.61 142.24 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 0 0 0))
  )
  (global_label "inp" (shape input) (at 127 111.76 0) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 0 0 0))
  )
  (global_label "inn" (shape input) (at 78.74 111.76 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 0 0 0))
  )
  (symbol (lib_id "pyopus:NMOS") (at 100.33 133.35 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Mn4" (id 0) (at 105.41 128.27 0))
    (property "Value" "" (id 1) (at 105.41 125.73 0))
    (property "Footprint" "" (id 2) (at 105.41 125.73 0))
    (property "Datasheet" "" (id 3) (at 100.33 133.35 0))
    (property "Model" "submodn" (id 4) (at 92.71 139.7 0))
    (property "w" "{mirr_wd}" (id 5) (at 99.06 128.27 0))
    (property "l" "{mirr_ld}" (id 6) (at 99.06 130.81 0))
    (property "m" "1" (id 7) (at 99.06 137.16 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (symbol (lib_id "pyopus:NMOS") (at 67.31 133.35 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Mn3" (id 0) (at 62.23 128.27 0))
    (property "Value" "" (id 1) (at 62.23 125.73 0))
    (property "Footprint" "" (id 2) (at 62.23 125.73 0))
    (property "Datasheet" "" (id 3) (at 67.31 133.35 0))
    (property "Model" "submodn" (id 4) (at 62.23 130.81 0))
    (property "w" "{mirr_w}" (id 5) (at 68.58 128.27 0))
    (property "l" "{mirr_l}" (id 6) (at 68.58 130.81 0))
    (property "m" "1" (id 7) (at 68.58 137.16 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (symbol (lib_id "pyopus:NMOS") (at 148.59 133.35 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Mn5" (id 0) (at 153.67 128.27 0))
    (property "Value" "" (id 1) (at 153.67 125.73 0))
    (property "Footprint" "" (id 2) (at 153.67 125.73 0))
    (property "Datasheet" "" (id 3) (at 148.59 133.35 0))
    (property "Model" "submodn" (id 4) (at 153.67 130.81 0))
    (property "w" "{mirr_wo}" (id 5) (at 147.32 128.27 0))
    (property "l" "{mirr_l}" (id 6) (at 147.32 130.81 0))
    (property "m" "1" (id 7) (at 147.32 137.16 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (symbol (lib_id "pyopus:PMOS") (at 91.44 83.82 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Mp1" (id 0) (at 86.36 88.9 0))
    (property "Value" "" (id 1) (at 86.36 91.44 0))
    (property "Footprint" "" (id 2) (at 86.36 90.17 0))
    (property "Datasheet" "" (id 3) (at 86.36 88.9 0))
    (property "Model" "submodp" (id 4) (at 86.36 86.36 0))
    (property "w" "{load_w}" (id 5) (at 92.71 88.9 0))
    (property "l" "{load_l}" (id 6) (at 92.71 86.36 0))
    (property "m" "1" (id 7) (at 92.71 80.01 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (symbol (lib_id "pyopus:PMOS") (at 114.3 83.82 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Mp2" (id 0) (at 119.38 88.9 0))
    (property "Value" "" (id 1) (at 119.38 91.44 0))
    (property "Footprint" "" (id 2) (at 119.38 90.17 0))
    (property "Datasheet" "" (id 3) (at 119.38 88.9 0))
    (property "Model" "submodp" (id 4) (at 119.38 86.36 0))
    (property "w" "{load_w}" (id 5) (at 113.03 88.9 0))
    (property "l" "{load_l}" (id 6) (at 113.03 86.36 0))
    (property "m" "1" (id 7) (at 113.03 80.01 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (symbol (lib_id "pyopus:PMOS") (at 148.59 83.82 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Mp3" (id 0) (at 153.67 88.9 0))
    (property "Value" "" (id 1) (at 153.67 91.44 0))
    (property "Footprint" "" (id 2) (at 153.67 90.17 0))
    (property "Datasheet" "" (id 3) (at 153.67 88.9 0))
    (property "Model" "submodp" (id 4) (at 153.67 86.36 0))
    (property "w" "{out_w}" (id 5) (at 147.32 88.9 0))
    (property "l" "{out_l}" (id 6) (at 147.32 86.36 0))
    (property "m" "2" (id 7) (at 147.32 80.01 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (symbol (lib_id "pyopus:ISRC") (at 64.77 100.33 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "I1" (id 0) (at 60.96 100.33 90))
    (property "Value" "" (id 1) (at 58.42 100.33 90))
    (property "Footprint" "" (id 2) (at 57.912 119.38 90))
    (property "Datasheet" "" (id 3) (at 59.69 119.38 90))
    (property "Specification" "dc={ibias}" (id 4) (at 68.58 100.33 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pyopus:RES") (at 146.05 99.06 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R1" (id 0) (at 146.05 96.52 90))
    (property "Value" "" (id 1) (at 146.05 93.98 90))
    (property "Footprint" "" (id 2) (at 146.05 97.282 90))
    (property "Datasheet" "" (id 3) (at 146.05 101.092 90))
    (property "r" "{r_out}" (id 4) (at 146.05 101.6 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pyopus:CAP") (at 135.89 99.06 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C1" (id 0) (at 135.89 95.25 90))
    (property "Value" "" (id 1) (at 135.89 92.71 90))
    (property "Footprint" "" (id 2) (at 132.08 100.0252 90))
    (property "Datasheet" "" (id 3) (at 135.89 95.25 90))
    (property "c" "{c_out}" (id 4) (at 135.89 102.87 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pyopus:NMOS") (at 86.36 111.76 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Mn1" (id 0) (at 91.44 106.68 0))
    (property "Value" "" (id 1) (at 91.44 104.14 0))
    (property "Footprint" "" (id 2) (at 91.44 104.14 0))
    (property "Datasheet" "" (id 3) (at 86.36 111.76 0))
    (property "Model" "submodn" (id 4) (at 91.44 109.22 0))
    (property "w" "{diff_w}" (id 5) (at 85.09 106.68 0))
    (property "l" "{diff_l}" (id 6) (at 85.09 109.22 0))
    (property "m" "1" (id 7) (at 85.09 115.57 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (symbol (lib_id "pyopus:NMOS") (at 119.38 111.76 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Mn2" (id 0) (at 114.3 106.68 0))
    (property "Value" "" (id 1) (at 114.3 104.14 0))
    (property "Footprint" "" (id 2) (at 114.3 104.14 0))
    (property "Datasheet" "" (id 3) (at 119.38 111.76 0))
    (property "Model" "submodn" (id 4) (at 114.3 109.22 0))
    (property "w" "{diff_w}" (id 5) (at 120.65 106.68 0))
    (property "l" "{diff_l}" (id 6) (at 120.65 109.22 0))
    (property "m" "1" (id 7) (at 120.65 115.57 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (symbol (lib_id "pyopus:SUBCKT") (at 176.53 101.6 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "A3" (id 0) (at 166.37 100.33 0))
    (property "Value" "" (id 1) (at 176.53 104.14 0))
    (property "Footprint" "" (id 2) (at 176.53 101.6 0))
    (property "Datasheet" "" (id 3) (at 176.53 101.6 0))
    (property "Name" "miller" (id 4) (at 166.37 107.95 0))
    (property "Pins" "inp inn out vdd vss" (id 5) (at 166.37 110.49 0))
  )
  (symbol (lib_id "pyopus:OUTPUT_FILE") (at 176.53 76.2 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "A1" (id 0) (at 166.37 74.93 0))
    (property "Value" "" (id 1) (at 176.53 78.74 0))
    (property "Footprint" "" (id 2) (at 176.53 76.2 0))
    (property "Datasheet" "" (id 3) (at 176.53 76.2 0))
    (property "Name" "miller.inc" (id 4) (at 166.37 82.55 0))
  )
  (symbol (lib_id "pyopus:INCLUDE") (at 176.53 88.9 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "A2" (id 0) (at 166.37 87.63 0))
    (property "Value" "" (id 1) (at 176.53 91.44 0))
    (property "Footprint" "" (id 2) (at 176.53 88.9 0))
    (property "Datasheet" "" (id 3) (at 176.53 88.9 0))
    (property "Filename" "mosmm.inc" (id 4) (at 166.37 95.25 0))
    (property "Position" "top" (id 5) (at 186.69 87.63 0))
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "A1") (unit 1) (value "OUTPUT_FILE") (footprint "")
    )
    (path
      (reference "A2") (unit 1) (value "INCLUDE") (footprint "")
    )
    (path
      (reference "A3") (unit 1) (value "SUBCKT") (footprint "")
    )
    (path
      (reference "C1") (unit 1) (value "CAP") (footprint "")
    )
    (path
      (reference "I1") (unit 1) (value "ISRC") (footprint "")
    )
    (path
      (reference "Mn1") (unit 1) (value "NMOS") (footprint "")
    )
    (path
      (reference "Mn2") (unit 1) (value "NMOS") (footprint "")
    )
    (path
      (reference "Mn3") (unit 1) (value "NMOS") (footprint "")
    )
    (path
      (reference "Mn4") (unit 1) (value "NMOS") (footprint "")
    )
    (path
      (reference "Mn5") (unit 1) (value "NMOS") (footprint "")
    )
    (path
      (reference "Mp1") (unit 1) (value "PMOS") (footprint "")
    )
    (path
      (reference "Mp2") (unit 1) (value "PMOS") (footprint "")
    )
    (path
      (reference "Mp3") (unit 1) (value "PMOS") (footprint "")
    )
    (path
      (reference "R1") (unit 1) (value "RES") (footprint "")
    )
  )
)
